_____________________________________________
  #####   ##   #####    ##
 ###     ###  ##       ###
  ###   # ## ##  #### # ##
   ### ##### ##    # #####
##### #   ##  ##### #   ##
_____________________________________________

library path:	D:\projects\sextante\workspaces\gvsig_1_11\_fwAndami\gvSIG\extensiones\es.unex.sextante\saga\modules
library name:	ta_morphometry
module name :	Multiresolution Index of Valley Bottom Flatness (MRVBF)
author      :	(c) 2006 by O.Conrad
_____________________________________________
go...
Usage: 8 -DEM <str> -MRVBF <str> -MRRTF <str> [-T_SLOPE <str>] [-T_PCTL_V <str>] [-T_PCTL_R <str>] [-P_SLOPE <str>] [-P_PCTL <str>] [-UPDATE] [-CLASSIFY] [-MAX_RES <str>]
  -DEM:<str>     	Elevation
	Grid (input)
  -MRVBF:<str>   	MRVBF
	Grid (output)
  -MRRTF:<str>   	MRRTF
	Grid (output)
  -T_SLOPE:<str> 	Initial Threshold for Slope
	Floating point
	Value Range: 0.000000 - 100.000000
  -T_PCTL_V:<str>	Threshold for Elevation Percentile (Lowness)
	Floating point
	Value Range: 0.000000 - 1.000000
  -T_PCTL_R:<str>	Threshold for Elevation Percentile (Upness)
	Floating point
	Value Range: 0.000000 - 1.000000
  -P_SLOPE:<str> 	Shape Parameter for Slope
	Floating point
  -P_PCTL:<str>  	Shape Parameter for Elevation Percentile
	Floating point
  -UPDATE        	Update Views
	Boolean
  -CLASSIFY      	Classify
	Boolean
  -MAX_RES:<str> 	Maximum Resolution (Percentage)
	Floating point
	Value Range: 0.000000 - 100.000000
